Author: Edmunds

SPEEDWAY / PACK LEADER
SPM-10 STAND APPLICATOR
SHOWN WITH OPTIONAL
CORNER WRAP
Stepper Driven
The SPM-10 Stand Applicator can be purchased with a head that
swivels for top or side labeling over a conveyor or fixed for
top or side labeling.
The SPM-10 is constructed of stainless steel and aluminum
and comes with swivel castors for ease of mobility
and leveling feet for final positioning.
Features: ~Touch Screen display for easy set up
~ Heavy duty Tee based stand (painted steel and
aluminum construction)
Specifications:
~110 VAC 50/60 HZ 1 PH
~Max. Dispensing Speed - 100’/min
~Max. 5 7/8” high label (OPTIONAL 7 7/8”)
~Max. web outer diameter - 14”
~3” inner core diameter
Optional:
~Ultrasonic clear label sensor
~Easy swivel pivot for top and side labeling
~8" high applicator
~Stainless steel stand

Speedway Packaging Machinery Inc.
www.spmi.ca